Gocator API

## ◆ GoMultiplexBank_HasSensor()

kBool GoMultiplexBank_HasSensor | ( | GoMultiplexBank | bank,
|  | k32u | id
| ) |  |

Returns a boolean value representing whether a sensor is in the multiplexing bank.

Version
  Introduced in firmware 4.0.10.27

Parameters

  bank | GoMultiplexBank object.
  id | The sensor ID to search for.

Returns
  kTRUE if the sensor is in the multiplexing bank, kFALSE otherwise.