Gocator API

## ◆ GoControl_BeginStart()

kStatus GoControl_BeginStart | ( | GoControl | control | ) |

Sends a start command to a sensor with the currently selected input source, but doesn't wait for the response.

Use the GoControl_EndStart function to wait for the sensor's reply.

Version
  Introduced in firmware 4.0.10.27

Parameters

  control | GoControl object.

Returns
  Operation status.

See also
  GoControl_EndStart, GoControl_SetInputSource, GoControl_GetInputSource