Gocator API

## ◆ GoSensor_SetRuntimeVariables()

kStatus GoSensor_SetRuntimeVariables | ( | GoSensor | sensor,
|  | kSize | startIndex,
|  | kSize | length,
|  | k32s * | values
| ) |  |

Sets the runtime variables from the provided starting index to the specified length with the values contained in the provided array.

Version
  Introduced in firmware 4.5.3.57

Parameters

  sensor | GoSensor object.
  startIndex | The starting index of the runtime variable values to set.
  length | The number of runtime variables to set/the length of the array parameter.
  values | A reference to an array which contains the intended runtime variable values.

Returns
  Operation status.