Gocator API

## ◆ GoSensor_ClearAlignment()

kStatus GoSensor_ClearAlignment | ( | GoSensor | sensor | ) |

Clears the current sensor alignment.

WARNING! This operation writes to flash storage. Review the user manual for implications.

Version
  Introduced in firmware 4.1.3.106

Parameters

  sensor | GoSensor object.

Returns
  Operation status.

See also
  GoSensor_Align

Remarks
  Calling this function will result in writing operations to flash storage. Should the process be disrupted due to power loss or other factors, the sensor may enter Rescue mode.