Gocator API

## ◆ GoControl_CopyFile()

kStatus GoControl_CopyFile | ( | GoControl | control,
|  | const kChar * | source,
|  | const kChar * | destination
| ) |  |

Copies a file within the connected sensor.

Version
  Introduced in firmware 4.0.10.27

Parameters

  control | GoControl object.
  source | Source name for the file to be copied.
  destination | Destination name for the file (maximum 63 characters).

Returns
  Operation status.