Gocator API

## ◆ GoSetup_SetIntensityMode()

kStatus GoSetup_SetIntensityMode | ( | GoSetup | setup,
|  | GoRole | role,
|  | GoIntensityMode | mode
| ) |  |

Sets the intensity data generation mode.

Version
  Introduced in firmware 4.7.10.10

Parameters

  setup | GoSetup object.
  role | Determines which sensor to apply changes to.
  mode | Intensity generation mode.

Returns
  Operation status.