Gocator API

## ◆ GoSetup_SetSpacingIntervalType()

kStatus GoSetup_SetSpacingIntervalType | ( | GoSetup | setup,
|  | GoRole | role,
|  | GoSpacingIntervalType | type
| ) |  |

Sets the spacing interval type.

Version
  Introduced in firmware 4.0.10.27

Parameters

  setup | GoSetup object.
  role | Determines which sensor to apply changes to.
  type | The spacing interval type.

Returns
  Operation status.