Gocator API

Public Member Functions
GoGeoCal Class Reference
GoSdk

## Description

Contains the GeoCal data for a sensor. Do not read the GeoCal file directly, use this class to parse it.

Inheritance diagram for GoGeoCal:

## Public Member Functions
kStatus | GoGeoCal_ApplyActiveArea (GoGeoCal cal, k32u x, k32u y, k32u width, k32u height, k32u xSubsampling, k32u ySubsampling, kSize cameraIndex)
| Applies a new camera window to the camera orientation information and updates coefficients. More...
kStatus | GoGeoCal_CalWindow (GoGeoCal cal, kSize cameraIndex, k32u *x, k32u *y, k32u *width, k32u *height, k32u *xSubsampling, k32u *ySubsampling)
| Gets calibration window. More...
kSize | GoGeoCal_CameraCount (GoGeoCal cal)
| Gets count of cameras. More...
k32u | GoGeoCal_Id (GoGeoCal cal)
| Gets sensor ID. More...
k64f | GoGeoCal_Roll (GoGeoCal cal, kSize cameraIndex)
| Gets camera roll angle. More...
const kChar * | GoGeoCal_Timestamp (GoGeoCal cal)
| Gets timestamp. More...
kArray1 | GoGeoCal_XCenterFit (GoGeoCal cal, kSize cameraIndex)
| Gets X center to Z fit. More...
kArray1 | GoGeoCal_XResolutionFit (GoGeoCal cal, kSize cameraIndex)
| Gets X resolution to Z fit. More...
kArray1 | GoGeoCal_YCenterFit (GoGeoCal cal, kSize cameraIndex)
| Gets Y center to Z fit. More...
kArray1 | GoGeoCal_YResolutionFit (GoGeoCal cal, kSize cameraIndex)
| Gets Y resolution to Z fit. More...

The documentation for this class was generated from the following file:

- GoGeoCal.h