Gocator API

## ◆ GoPartDetection_SetEdgeFilterLength()

kStatus GoPartDetection_SetEdgeFilterLength | ( | GoPartDetection | detection,
|  | k64f | value
| ) |  |

Sets the part detection edge filtering Length.

Version
  Introduced in firmware 4.2.4.7

Parameters

  detection | GoPartDetection object.
  value | The part detection edge filtering length value to set.(mm)

Returns
  Operation status.