Gocator API

## ◆ GoControl_BeginUpgrade()

kStatus GoControl_BeginUpgrade | ( | GoControl | control,
|  | void * | data,
|  | kSize | size
| ) |  |

Begins a sensor firmware upgrade.

Use the GoControl_GetUpgradeStatus function to poll for upgrade completion.

Version
  Introduced in firmware 4.0.10.27

Parameters

  control | GoControl object.
  data | Pointer to buffer containing upgrade file.
  size | Size of upgrade file.

Returns
  Operation status.

See also
  GoControl_GetUpgradeStatus