Gocator API

## ◆ GoControl_WriteFile()

kStatus GoControl_WriteFile | ( | GoControl | control,
|  | const kChar * | fileName,
|  | const kByte * | data,
|  | kSize | size
| ) |  |

Writes a file to the connected sensor.

Version
  Introduced in firmware 4.0.10.27

Parameters

  control | GoControl object.
  fileName | Name of remote file to be written.
  data | Pointer to buffer containing the file data.
  size | Size of the file.

Returns
  Operation status.