Gocator API

## ◆ GoAnalog_SetDelay()

kStatus GoAnalog_SetDelay | ( | GoAnalog | analog,
|  | k64s | delay
| ) |  |

Sets the delay from exposure until output is triggered, in units based on GoDomain mm when GoDomain is distance, uS when GoDomain is time.

The delay is ignored when GoDomain is Immediate or when output is Software triggered.

Version
  Introduced in firmware 4.0.10.27

Parameters

  analog | GoAnalog object.
  delay | The delay (uS or mm)

Returns
  Operation status.