Gocator API

## ◆ GoTransform_SetY()

kStatus GoTransform_SetY | ( | GoTransform | transform,
|  | GoRole | role,
|  | k64f | offset
| ) |  |

Sets the transformation Y component.

Version
  Introduced in firmware 4.0.10.27

Parameters

  transform | GoTransform object.
  role | The sensor role transformation entry to update.
  offset | The transformation Y component to set.

Returns
  Operation status.