Gocator API

## ◆ GoSetup_ActiveAreaHeightLimitMax()

k64f GoSetup_ActiveAreaHeightLimitMax | ( | GoSetup | setup,
|  | GoRole | role
| ) |  |

Gets the maximum valid value for the ActiveAreaHeight setting.

Version
  Introduced in firmware 4.0.10.27

Parameters

  setup | GoSetup object.
  role | Determines which device to retrieve the value from.

Returns
  Maximum valid active area height value (mm).