Gocator API

## ◆ GoTracheid_GetCameraThresholdAt()

kStatus GoTracheid_GetCameraThresholdAt | ( | GoTracheid | tracheid,
|  | kSize | cameraIndex,
|  | k32s * | threshold
| ) |  |

Gets the camera threshold.

Version
  Introduced in firmware 4.5.3.57

Parameters

  tracheid | GoTracheid object.
  cameraIndex | Camera index (0 or 1).
  threshold | A reference to be updated with the threshold value.

Returns
  Operation status.