Gocator API

## ◆ GoSetup_EnableIndependentExposures()

kStatus GoSetup_EnableIndependentExposures | ( | GoSetup | setup,
|  | GoRole | role,
|  | kBool | enable
| ) |  |

Enables independent exposures feature, i.e.

separate exposures for separate cameras.

Version
  Introduced in firmware 4.6.0.140

Parameters

  setup | GoSetup object.
  role | Determines which sensor to apply changes to.
  enable | kTRUE to enable, or kFALSE to disable.

Returns
  Operation status.