Gocator API

## ◆ GoSetup_SetPatternSequenceType()

kStatus GoSetup_SetPatternSequenceType | ( | GoSetup | setup,
|  | GoRole | role,
|  | GoPatternSequenceType | type
| ) |  |

Sets the pattern sequence type.

Version
  Introduced in firmware 4.2.4.7

Parameters

  setup | GoSetup object.
  role | Determines which sensor to apply changes to.
  type | The pattern sequence type to set.

Returns
  Operation status.