Gocator API

## ◆ GoEthernet_RemoveCompositeSource()

kStatus GoEthernet_RemoveCompositeSource | ( | GoEthernet | ethernet,
|  | GoOutputSource | type,
|  | kSize | index
| ) |  |

Removes (deselects) the composite source at the specified index.

Version
  Introduced in firmware 4.4.4.14

Parameters

  ethernet | GoEthernet object.
  type | Output type.
  index | Index of the composite source to be removed.

Returns
  Operation status.