Gocator API

## ◆ GoTransform_SetYAngle()

kStatus GoTransform_SetYAngle | ( | GoTransform | transform,
|  | GoRole | role,
|  | k64f | offset
| ) |  |

Sets the transformation Y-angle.

Version
  Introduced in firmware 4.0.10.27

Parameters

  transform | GoTransform object.
  role | The sensor role transformation entry to update.
  offset | The transformation Y-angle to set in degrees

Returns
  Operation status.