Gocator API

## ◆ GoAnalog_EnableCurrentInvalid()

kStatus GoAnalog_EnableCurrentInvalid | ( | GoAnalog | analog,
|  | kBool | enable
| ) |  |

Enables the current output level associated with an invalid measurement.

When this is disabled, the output value will be held constant on an invalid measurement

Version
  Introduced in firmware 4.0.10.27

Parameters

  analog | GoAnalog object.
  enable | kTRUE to enable, or kFALSE to disable.

Returns
  Operation status.