Gocator API

## ◆ GoSensor_GetFlag()

kStatus GoSensor_GetFlag | ( | GoSensor | sensor,
|  | const kChar * | name,
|  | kString | value
| ) |  |

Gets a sensor flag value.

See GoSensor_SetFlag for more details.

Version
  Introduced in firmware 5.2.18.3

Parameters

  sensor | GoControl object.
  name | Name of the flag.
  value | String object to receive the value (in text).

Returns
  Operation status.