Gocator API

## ◆ GoSetup_SetXSubsampling()

kStatus GoSetup_SetXSubsampling | ( | GoSetup | setup,
|  | GoRole | role,
|  | k32u | xSubsampling
| ) |  |

Sets the current x-resolution divider.

Version
  Introduced in firmware 4.0.10.27

Parameters

  setup | GoSetup object.
  role | Determines which sensor to apply changes to.
  xSubsampling | X subsampling divider (e.g. 1 - full res, 2 - half res).

Returns
  Operation status.