Gocator API

## ◆ GoSetup_FrontCameraExposureLimitMin()

k64f GoSetup_FrontCameraExposureLimitMin | ( | GoSetup | setup,
|  | GoRole | role
| ) |  |

Gets the minimum valid value for the front camara exposure setting.

Version
  Introduced in firmware 4.6.0.140

Parameters

  setup | GoSetup object.
  role | Determines which device to retrieve the value from.

Returns
  Minimum valid auxiliary exposure value (microseconds).