Gocator API

## ◆ GoSetup_IntensitySourceOptionAt()

GoIntensitySource GoSetup_IntensitySourceOptionAt | ( | GoSetup | setup,
|  | GoRole | role,
|  | kSize | index
| ) |  |

Gets the intensity source option at the given index.

Version
  Introduced in firmware 4.6.0.152

Parameters

  setup | GoSetup object.
  role | Determines which device to retrieve the value from.
  index | The index with which to retrieve an exposure mode option.

Returns
  Intensity source set.

See also
  GoSetup_IntensitySourceOptionCount