Gocator API

## ◆ GoSurfaceGenerationFixedLength_SetTriggerExternalInputIndex()

kStatus GoSurfaceGenerationFixedLength_SetTriggerExternalInputIndex | ( | GoSurfaceGeneration | surface,
|  | k32s | index
| ) |  |

Sets the external input index to trigger surface capturing.

Version
  Introduced in firmware 5.2.1.110

Parameters

  surface | GoSurfaceGeneration object.
  index | External digital input index.

Returns
  Operation status.