Gocator API

## ◆ GoSetup_SetFrontCameraExposure()

kStatus GoSetup_SetFrontCameraExposure | ( | GoSetup | setup,
|  | GoRole | role,
|  | k64f | exposure
| ) |  |

Sets the front camera exposure value.

Version
  Introduced in firmware 4.6.0.140

Parameters

  setup | GoSetup object.
  role | Determines which sensor to apply changes to.
  exposure | Intended auxiliary exposure value.

Returns
  Operation status.