Gocator API

## ◆ GoSensor_AccelOpMode()

GoDiscoveryOpMode GoSensor_AccelOpMode | ( | GoSensor | sensor | ) |

Returns the operational mode of the sensor.

This can be used by an acceleration application to determine if the sensor is a virtual sensor, standalone sensor or an accelerated sensor mode.

Version
  Introduced in firmware 5.2.18.3

Parameters

  sensor | GoSensor object.

Returns
  Sensor operational mode.