Gocator API

## ◆ GoSetup_ExposureStepAt()

k64f GoSetup_ExposureStepAt | ( | GoSetup | setup,
|  | GoRole | role,
|  | kSize | index
| ) |  |

Get the exposure step value specified by index.

Version
  Introduced in firmware 4.0.10.27

Parameters

  setup | GoSetup object.
  role | Determines which device to retrieve the value from.
  index | The index of the exposure step to get.

Returns
  The exposure step value (microseconds).

See also
  GoSetup_ExposureStepCount