Gocator API

## ◆ GoSensor_SetDefaultJob()

kStatus GoSensor_SetDefaultJob | ( | GoSensor | sensor,
|  | const kChar * | fileName
| ) |  |

Sets a default job file to be loaded on boot.

WARNING! This operation writes to flash storage. Review the user manual for implications.

Version
  Introduced in firmware 4.0.10.27

Parameters

  sensor | GoSensor object.
  fileName | Name of the default file.

Returns
  Operation status.

Remarks
  Calling this function will result in writing operations to flash storage. Should the process be disrupted due to power loss or other factors, the sensor may enter Rescue mode.