Gocator API

## ◆ status

k64u GoStamp::status

Bit mask containing frame information:

- Bit 0: Represents sensor digital input state.
- Bit 4: Represents Master digital input state.
- Bits 8 and 9: Represents inter-frame digital pulse trigger (Master digital input if a Master is connected, otherwise sensor digital input. Value is cleared after each frame and clamped at 3 if more than 3 pulses are received).